

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Nano** - for all pistons | **Micro** piston  small turbines | **Mini** larger  turbines | **Maxi**  large  turbines | **Turbinator**  biggest |
| AH Capacity | 9 | 12 | 16 | 30 | 40 |
| Wh Energy | 189 | 324 | 432 | 810 | 1080 |
| Voltage – freshly charged | 29.2 | 29.2 | 29.2 | 29.2 | 29.2 |
| Voltage - Nominal | 26.8 | 26.8 | 26.8 | 26.8 | 26.8 |
| Max Current Pulse Amps | 700 | 1000 | 2000 | 2600 | 3500 |
| Max continuous Amps | 250 | 250 | 350 | 450 | 500 |
| Terminal IR / Impedance | 12.6 | 9.3 | 8.3 | 6.9 | 2.9 |
| Specific Power KW ( E x I ) | 8kw | 13kw | 21kw | 38kw | 48kw |
| **WEIGHT / MASS lb / kg** | **2.2 / 1** | **3.0 / 1.5** | **7.0 / 3.2** | **10 / 4.5** | **11 / 5.0** |
| Dimensions | 5x3x3 | 8x3x3 | 9x6x3 | 11x6x3 | 16x5x4 |
| # of starts | 2 - 3 | 2 - 3 | 2 - 3 | 2 - 3 | 2 - 3 |
| Charge / Start cycles x 1000 | 3 - 4 | 3 - 4 | 3 - 4 | 3 - 4 | 16 - 20 |
| Recharge time in minutes @ 5A | > 1st start - | 30 min. | > 2nd – 60 | > 3rd - 120 | ***5 minutes*** |
| Operating temps F | 30 - 150 | 30 - 150 | 30 - 150 | 30 - 150 | 5 - 150 |
| Torque load on connector ft/lbs | 1 | 2 | 5 | 7 | 7.7 |
| Investment $$ - Includes hard case, charger and ***BLUEtooth*\*** | 375 | 1500 | 2500\* | 3500\* | 4000\* |
| Compare $ to; startpac/start-stick | X / X | X / 3545 | 2973 / 4450 | 4522 / 5495 | X / X |

Advantages over other older portable units;

Higher voltage maintained under load, 23-24v vs. 18-19

Much less torquing on 3 pin connector

THE smallest and lightest portable starting GPU’s on the market!

Utilizing the newest cell tech

Very safe, non hazardous, zero maintenance

Impact resistant aluminum and polycarbonate cases

Bluetooth monitoring on Mini, Maxi, and Turbinator models